**Tender text**

**Franke cup warmer CW270**

For all product lines of the A-, S- and SB-series

The cup warmer is designed for storage and preheating of cups and glasses for the preparation of coffee specialties.

**Technical data**

Cup warmer: 4 trays: up to 120 Cups

Mains power connection: 220-240 VAC, 1L N PE, 110-130W, 50-60 Hz

 110-127 VAC, 1L N PE, 80-130W, 50-60 Hz

 100 VAC, 1L N PE, 80W, 50-60 Hz

 220 VAC, 1L N PE, 110W, 50-60 Hz

Empty weight: up to max. 20 kg

Dimensions: Width: 270 mm

 Hight: 544 mm (with feet 7 mm – standard for A200)

 Hight: 585 mm (with feet 40 mm– standard

A- and S-series except A200)

 Depth: 453 mm

Approvals: CE / CB

**Device design**

All essential parts are made of stainless steel. The housing parts are made of easy-care plastic.

**Features**

The cup warmer with 4 heatable trays for the storage of coffee cups is adapted to the design of the coffee machine. It can be installed on the left or right side and can be fixed at the coffee machine. Even stand-alone is possible. Separate main switch on the front. The temperature is factory set and is regulated by a thermostat.

**Manufacturer** Franke Kaffeemaschinen AG (ISO 9001 certified)