# Tender text

# Tank kit with external water pump

For product lines A300, A400, A600, A800, A1000, S700, SB1200.

External water pump incl. fresh- and wastewatertank for mobile water supply of a coffee machine with water connection and drain hose on the drip tray.

## Diaphragm pump:

Dimensions: W 130 mm x H 210 mm x D 80 mm

Mains power connection: 12 VDC 1,2À / 230 VAC 1LNPE, 50 W, 10 A, 50/60 Hz

Water inlet: Diameter 9,5 mm (3/8”)

Water outlet: Diameter 9,5 mm (3/8”)

Weight (pump): 2,0 kg

Noise emission: < 70 dB (A)

Approvals: CE

**Tanks:**

Dimensions: W 232 mm x H 412 mm (app. 500 mm with level sensors) x D 280 mm.

 Volume 16 l each

**Control Unit:**

Dimensions: W 98 mm x H 55 mm x D 28 mm

## Features

## Dry-running safe and self-priming pump in plastic housing with thermal overload protection. Separate switch to disconnect the pump from the mains. Delivery ready to plug in incl. power adapter. Fresh water tank with empty alarm device, waste water tank with full alarm device. Display of messages on the display of the connected coffee machine. Both tanks are made of plastic, with carrying handle and separate lid. The tank kit is suitable for installation in the mobile coffee cart or in the counter base

**Manufacturer** Franke Kaffeemaschinen AG (ISO 9001 certified)