# Tender Text

# Coffee Cart KW

For product lines A300, A400, A600, A800, A1000, S700, SB1200.

Mobile substructure for a mobile coffee station for decentralized, flexible coffee supply indoors.

## Technical data

Ultimate load: max. 150 kg

Rollers: 4 Swivelcastors, Ø 125 mm, lockable, Running surface thermoplastic rubber

Weight: Module basic: 43 kg

Module cup dispenser: 21 kg

Module waste container: 25 kg

Module storage shelve: 6 kg

Dimensions: Module basic: B: 650 mm H: 910 mm T: 650 mm

Module cup dispenser: B: 240 mm H: 762 mm T: 701 mm

Module waste container: B: 370 mm H: 762 mm T: 650 mm

Module storage shelve: B: 410 mm H: 42 mm T: 650 mm

**Module basic:**

Version in powder-coated sheet steel. The side panels and the partition between the operating and service sides are perforated. Colour matt black RAL 9005 fine structure. Door on the operating side with recessed handle. Door service side. Both lockable with cylinder lock. Both shelves are made of galvanized steel. Variable cover plate designs and arrangements for different equipment constellations as well as with and without holes for supply lines and coffee ground ejection. Openings for cable feedthroughs in the floor and partition. Mounting option on the service side of e.B. water filter and water pump on the perforated partition wall between the operating and service side. Holder for tanks for water supply or water disposal as well as the container for coffee grounds ejection on the operating side. Possibility of expansion on the left and right side by one optional mounting module each.

**Module cup dispenser (Option):**

Version in powder-coated sheet steel. Colour matt black RAL 9005 fine structure. Mounting on the right and left side of the basic module possible. Extension of the work surface by 240 mm in width. Three integrated, adjustable cup tubes for cup sizes from 0.2 to 1.04 liters.

**Module waste container (Option):**

Version in powder-coated sheet steel. Colour matt black RAL 9005 fine structure. Mounting on the right and left side of the basic module possible. Extension of the work surface by 370 mm in width. Insertion flap for waste in the door. Door lockable with cylinder lock. Integrated waste container with a volume of 27 liters.

**Module storage shelf (Option):**

Stainless steel version. Mounting on the right and left side of the basic module possible. Extension of the work surface by 410 mm in width. 90° foldable via release lever under the storage area. Not approved for the installation of coffee machines or add-on units.

Application:

Only suitable for indoor use with flat floors. Not suitable for operation with Twin-Systems, cooling units placed under the counter and placed under the coffee machine.

**Manufacturer** Franke Kaffeemaschinen AG (ISO 9001 certificated)