Tender text

Franke add-on unit Flavor Station FS30

For product types A600 FM EC, A600 FM CM, A800 FM EC.

The add-on unit Flavor Station FS30 enables the automated and constant dosing of syrup in the coffee / milk spout of the coffee machine. The open system is designed for the use of syrup bottles in different sizes from different manufacturers. Each type of syrup is dosed in a closed system. An unwanted mixing of different syrups is therefore excluded**.** On top of the device is a heatable tray for the storage of cups.

Technical data

Storage: max. 3 bottles

Mains power connection: 220-240 VAC, 1L N PE, 50-60 Hz - CH/EU/GB

110-127 VAC, 1L N PE, 50-60 Hz - USA

 100 VAC, 1L N PE, 50-60 Hz - JP

 220 VAC, 1L N PE, 50 Hz - CN

Empty weight: max. 17 kg

Dimensions: Width: 200 mm

 Height: 586 mm (option – feet 7 mm)

Height: 625 mm (standard – feet 40 mm)

 Depth: 452 mm

Approvals: CE / CB

Device design

All essential parts are made of stainless steel. The housing parts are made of easy-care plastic. The heatable tray for the storage of cups is made of aluminium. The device front is made of glass.

Features

The flavor station is adapted to the design of the coffee machine and must be installed on the right side and can be fixed at the coffee machine. 3 separate dosing systems for up to 3 different sorts of syrups ensure the optimum dosage of the quantity of syrup. A message is displayed on the touchscreen of the coffee machine by the lack of syrup. The max. height of the syrup bottles is 310 mm. They are fixed in the lockable drawer. The adapters of the bottles are universally with diameters from 18 to 22 mm. 2 separate main switches located on the rear panel.

**Customer settings**

Customers can adjust parameters as for example the quantity of syrup via the touchscreen of the coffee machine. The backup of the product settings is carried out on the internal memory or via the usb interface. The access can be individually defined and secured with PIN-code.

**Billing systems**

Product billing of the prepared products is possible via the connected coffee machine which can be connected to commercial billing systems such as a coin validator, coin changer or card reader via an MDB interface. Integrated counters in the coffee machine per product purchase and total product purchase.

**Cleaning**

The integrated, automatic rinsing and cleaning program of the coffee machine makes maintaining the device easier. Visual user guide and display of cleaning steps on the touch screen of the coffee machine.

**Manufacturer** Franke Kaffeemaschinen AG (ISO 9001 certified)