**Tender text**

**Franke under counter Flavor Station FSU30**

For product types A600 FM EC, A600 FM CM, A800 FM EC

The under counter Flavor Station FSU30 enables the automated and constant dosing of syrup in the coffee / milk spout of the coffee machine. The open system is designed for the use of syrup bottles in different sizes from different manufacturers. Each type of syrup is dosed in a closed system. An unwanted mixing of different syrups is therefore excluded.

Technical data

Storage: max. 3 bottles

Mains power connection: 220-240 VAC, 1L N PE, 50-60 Hz - CH/EU/GB

110-127 VAC, 1L N PE, 50-60 Hz - USA

100 VAC, 1L N PE, 50-60 Hz - JP

220 VAC, 1L N PE, 50 Hz - CN

Net weight: up to max. 12 kg

Dimensions: Width: 235 mm

Hight: 420 mm

Depth: 350 mm

Approvals: CE / CB

Device design

All essential parts are made of stainless steel.

Features

The flavor station must be installed in the counter under the coffee machine. 3 separate dosing systems for up to 3 different sorts of syrups ensure the optimum dosage of the quantity of syrup. A message is displayed on the touchscreen of the coffee machine by the lack of syrup. The max. height of the syrup bottles is 400 mm. The max. diameter of the bottles is 85 mm. They are fixed in a separate drawer. The adapters of the bottles are universally with diameters from 18 to 22 mm. The Flavor Station unit has a separate main switch. The Flavor Station is located on 6 rolls with sliding direction forward/back.

Customer settings

Customers can adjust parameters as for example the quantity of syrup via the touchscreen of the coffee machine. The backup of the product settings is carried out on the internal memory or via the usb interface. The access can be individually defined and secured with PIN-code.

Billing systems

Product billing of the prepared products is possible via the connected coffee machine which can be connected to commercial billing systems such as a coin validator, coin changer or card reader via an MDB interface. Integrated counters in the coffee machine per product purchase and total product purchase.

Cleaning

The integrated, automatic rinsing and cleaning program of the coffee machine makes maintaining the device easier. Visual user guide and display of cleaning steps on the touch screen of the coffee machine.

**Manufacturer:** Franke Kaffeemaschinen AG (ISO 9001 certified)