**Specification text**

**Franke cup warmer**

For product lines Spectra and FoamMaster

The cup warmer is designed for storage and preheating of cups and glasses for the preparation of coffee specialties

Technical data

Cup warmer: 3 trays: up to 120 Cups

Electrical connection 220 -240 V, 1LNPE, 300 W, 10 A, 50/60 Hz

Net weight: up to max. 17 kg

Dimensions: Width: 300 mm

Hight: 570 mm (with standard feet)

Depth: 580 mm

Approvals: CE / CB / EMV

Device design

All essential parts are made of stainless steel. The housing parts are corrosion-protected.

Features

The cup warmer with 3 heatable trays for the storage of coffee cups, drip tray and drip grit is adapted to the design of the coffee machine. It can be installed on the left or right side of the coffee machine. Even stand-alone is possible. Separate main switch on the front. The temperature is factory set and is regulated by a thermostat.

**Manufacturer:** Franke Kaffeemaschinen AG (ISO 9001 certified)